The Furuno NX-700 product is a NAVTEX performance standard compliant, dual-channel reciever for SOLAS ships. It is capable of recieving two channels simultaneously, at 518 kHZ for international NAVTEX messages and from 490 to 4209.5 kHZ for domestic NAVTEX messages. Messages included are Navigational Warnings, Meteorological Warnings, Search and Rescue information, and local ship traffic. Broadcast stations may be automatically selected based on ship position with a GPS navigator. 
	Incoming messages are stored as non-volatile, meaning they can be maintained without power. Three font sizes are available for the 5" bright LCD screen. An external Serial (RS-232) printer can be connected to the compact and stylish NX-700 units (Display, Reciever, and H-Field Antenna) for convienent message printing. The H-field antenna requires no grounding and no extra whip antenna to provide reliable reception. Low power requirements of a 12-24 VDC and .7-.4A are needed for this system.